Input QSO spectra

Window size and marker number = forest region values

Window size and marker number = post values

Calculate markers in sliding window for:

Add markers at emission lines and end points

Calculate markers in sliding window for:

If:

pixels

True

False

Output continuum markers